|  |  |  |  |
| --- | --- | --- | --- |
| Course Name: | **Elements of Electrical and Electronics Engineering Laboratory** | **Semester:** | **I/II** |
| **Date of Performance:** | **/ / 20--** | **Batch No:** |  |
| **Student Name:** |  | **Roll No:** |  |
| **Faculty Sign & Date:** |  | **Grade/Marks:** | **/ 20** |

**Experiment No: 7**

**Title:** **Measurement of Power using Two Wattmeter Method**

|  |
| --- |
| **Aim and Objective of the Experiment:** |
| * To measure the power of three phase power using Two Wattmeter Method |

|  |
| --- |
| **COs to be achieved:** |
| **CO2:** Demonstrate and analyze steady state response of single phase and three phase circuits |

|  |
| --- |
| **Circuit Diagram:** |
|  |

|  |
| --- |
| **Stepwise-Procedure:** |
| 1. 1.Connect the circuit as shown in circuit diagram 2. 2. Increase the load and note down the reading VL,IL,W1 and W2 3. 3. Practically you will obtain total power W=W1+W2 4. 4. Theoretically power is measured by using formula P=√3VLILcosϕ,   using cosϕ=1(unity) for resistive load. |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Observation Table:**   |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **Sr.no** | **VL (Volts)** | **IL**  **(Amp)** | | **W1**  **(KW)** | | **W2**  **(KW)** | | **W= (W1+W2)**  **(KW)** | | | **P = √3VLILCOSϕ (KW)** | **Lamp**  **load given from lamp bank**  **(KW)** | |  |  | **TH** | **PR** | **TH** | **PR** | **TH** | **PR** | | **TH** | **PR** |  |  | | 1 |  |  |  |  |  |  |  | |  |  |  |  | | **2** |  |  |  |  |  |  |  | |  |  |  |  | | **3** |  |  |  |  |  |  |  | |  |  |  |  | | **4** |  |  |  |  |  |  |  | |  |  |  |  |   **Theoretical Calculations:**  **Power= x VL x IL x cos φ**  **cos φ=1**  **Power =Wattage rating of lamp load x No of lamps (One lamp is of 100W rating)**  **W1= VL x IL x cos (30+φ)**  **Φ=0**  **W2= VL x IL x cos (30-φ)**  **Total Power=P=W1+W2** |

|  |
| --- |
| **Conclusion:** |
|  |

|  |
| --- |
| **Signature of faculty in-charge with Date:** |